# CAMS-1 Quick Start (Church)

1. Place **stand** on flat floor; extend to aiming height; tighten clutch.  
2. Mount **speaker** on pole (M20 / 35 mm — match your hardware). Attach safety strap if in an aisle.  
3. Connect **XLR** from mixer main / aux / vocal subgroup.  
4. Connect **IEC** mains (earth required). Power ON — wait ~1 s through mute.  
5. Set HF trim to center; raise master slowly while pastor speaks.  
6. Walk the room; adjust aim and level for even speech at rear pews.

Full safety: `docs/safety.md` · Placement: `docs/placement-spl.md`
