# Recommended premium component set (order-ready)

Super-quality default kit for one CAMS-1 + stand. Alts listed where church durability may prefer pro drivers.

## Drivers (choose one tier)

| Tier | Midbass | Tweeter | Character |
|------|---------|---------|-----------|
| **Audiophile (default)** | Scan-Speak 32W/8878T00 | Scan-Speak D2608/913000 | Smooth vocals, low coloration |
| Alt hi-fi | Seas W22NY001 | Seas 27TFFNC/G | Excellent value premium |
| Alt installed-sound | B&C 8PE21 | BMS 4540 or peer 1″ | Higher SPL / touring toughness |

## Amplification & XO

- 2 × **LM3886TF/NOPB** (isolated tab)  
- 2 × **OPA2134** for LR4 @ 2.5 kHz  
- **THAT1200** or **INA134** balanced input  
- Toroid **2×22 V / 200 VA** (Antek AN-2220 class)  

## Connectors / hardware

- Neutrik **NCJ6FI-S** combo  
- Schaffner **FN9222** IEC  
- Adam Hall / generic **pole cup** matching stand  

## Cabinet

- Baltic birch 18 mm + 25 mm baffle  
- Matte durable finish  

## Stand

- Ø450 × 8 mm base, Ø35/30 telescopic, powder coat, ballast  

Exact lines: [`../bom/MASTER_BOM.csv`](../bom/MASTER_BOM.csv)

**VERIFY** every cutout and mains primary before production batch.
